**Controller Functions**

**Menu Path**

|  |  |
| --- | --- |
| Silence Alerts | Menu > 1 > 1 > 1 |
| Set Server IP | Menu > 2 > 2 > enter IP > Enter > Yes |
| Connect a Router | Plug in USB and Ethernet cables |
| Connect to Server | Menu > 2 > 1 > 1 |
| Manual Time Sync | Menu > 4 > 1 > enter new time (Date: YYYY/MM/DD, 24hr) > Enter > Yes |
| Use ChronoSync (wait for beep on insert) | Menu > 4 > 3 > 1 |
| Gun Start | Press Gun Start button |
| Marker | Menu > 1 > 2 > 1 |
| Event/Point Name Change | Menu > 1 > 3 > 1 > Shift to use Alpha > enter name > Enter > Yes |
| Set Active Extension Power Level | Menu > 8 > 1 |
| Set Active Extension Channel Number | Menu > 8 > 2 |
| Set Active Extension Loop ID | Menu > 8 > 3 > 1 |
| Reset Active Extension | Menu > 8 > 5 |
| Turn UHF On/Off (Gators and FPs) | Menu > 8 > 6 |
| USB File Copy (wait for beep on insert) | Menu > 3 > 2 > 1 (copy current) |
|  |  |
|  |  |

**Server and Login Info**

|  |  |
| --- | --- |
| Primary Server IP | 50.17.233.218 |
| Backup Server IP | 50.17.239.204 |
| Server Login (for SimpleClient/Timer Portal) |  |
| Server Password |  |
| CT Live Login |  |
| CT Live Password |  |
| Scoring Computer IP | 172.20.23. |
|  |  |
|  |  |

**Things to Watch**

|  |  |
| --- | --- |
| Battery Status | Battery LEDs |
| Errors/Alerts | Menu > 1 > 1 > 1 |
| Read Counts | Main Screen |
| Port Status | LEDs above cable ports |
|  |  |